Note from reviving the system

# 5/9/21

# Pump

Pump beam fiber was unstable and caused some problems. This led to TA not working. After re-coupling the fiber with costa everything got back to work.

# Coils calibration

Found at

E:\NMRGGil\scheme\_3\_home\static\_code\hw\_utils\coils magnetic calibration\toy\_script\_.m